ITEM #0979004A – Construction barricade detectable

*Section 9.79 is supplemented and amended as follows:*

**09.79.01—Description:**

*Replace the entire Article with the following:*

Under this item the Contractor shall furnish all Construction Barricade Detectable required on the Project as stated in the item “Maintenance and Protection of Traffic,” as shown on the plans, and as directed by the Engineer.

The Construction Barricade Detectable shall conform to the following:

1. have continuous detectable bottom and top surfaces able to be detected by a person with a visual disability traveling with the aid of a long cane;
2. the bottom of the bottom surface shall be no higher than 2 inches above the ground;
3. the top of the top surface shall be no lower than 32 inches above the ground;
4. the requirements of the 2016 AASHTO MASH.

**09.79.02—Materials:**

*Delete the last sentence and add the following:*

Prior to using Construction Barricade Detectable on the Project, the Contractor shall submit to the Engineer a copy of the Eligibility Letter issued by the FHWA to the manufacturer documenting that the barricades comply with the requirements of the 2016 AASHTO MASH and are eligible for reimbursement under the Federal-aid highway program.

**Pay Item** **Pay Unit**

Construction Barricade Detectable ea.