INI Revisions
XXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXX
May 3
created two separate v8 environments
2006 has leroy text
2007 has verdana + working text, new bdr size



Feb 7 2006
V3 
1.	Bin Report on Roadway Modeler turn off
2.	Bearings offset to bottom center 
3.	Feature for cut symb. Set for level HR_FEAT-cut
4.	BCLC feature line segments turned on in plan view
5.	Centerline feature line segments turn off in plan view
6.	Changed feature front of conc. Walk bench_rt to P_wlk, Sym P_buffer to breakline
7.	Updated tml
8.	Renamed INI to V4


Sept 25 2006
V4
1. Revised Options settings
	-Set A highway perference for UnitsTolerances Positional=1, Chord Height=1
		The default is set to .001 for chord ht as requested be surveys
	-Refesh command Settings on Preference Change ON
	-.12 decimal places set for N & E

2. Added symbology
	-P_ALG_H INTERSECTION COOR.
	-IND CON and INT CON
	-P_ALG H BEARING

3. Resised Horizantal Alignment Annotation
	-PI tangent turned off
	-Added NE PI coor to Curve data
	-PC STA. 10+00 changed to PC STA 10+00
	-Northing and Easting symbology set up.  Go to Geomentry>View Geometry>Station Base/clearance Annotation
	-Beaing set to standard

3. Revised all create cross section preferances
	-Station and elevation range off in create cross section and create profile
	-Cross section cell has a locked level so they can not be easily deleted
	-Create cross section features Include Features was turned ON
	-Window clearence forcross section, bottom changed to 15

4. Annotate profile revised
	-superelevation annotation was updated

5. Vertical annotation updated
	-Symbology is set for event Points

6. View surface updated
	-Added existing contour preference for veiwing contours

7. SURFACE > VEIW SURFACE 
	-Two point symbology annotation set

8. Existing Drainage Features
	-Added Profile symblogy and annotation for all existing drainage pipes and CBs
	-Added xsec symblogy and annotation for all existing drainage pipes, CB no option for project or ban with available in 8.5

9. Plan and Profile generator set up


Oct 02 2006
fwf and fxp v2
RevisionsOverhang chanded to exclude feature as dtm type.  


Nov 17 2006
ini V5
Separated CT Civil ini
Highways   CT_civil85_v5.ini - Set default perference for Units Tolerances Positional=1, Chord Height=1
		
surveys    SV_civil85_v5.ini - Set default perference for Units Tolerances Positional=1, Chord Height=.001

XXXXXXXXXXXXXXXXXXXXXXXX MAY 3 XXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXX
June 18 2007
John fixed fxp and fwf put V3 in 2006 


Sept 21 2007
INI set to Version 5a
Perimeter advance tab scale = 1 set for existing surface preference.


Jan 16 2008
Version 5b
Existing surface preference set to survey levels for Parimeter and Triangles
Existing suface prefence set up for Contours
Default for Parimeter, Triangles, contour all set to sym o,o,o


Jan 22, 2008
Set existing surface per & Tria. by-levels for all attributes

Jan 25, 2008
Version 5c
Added Facility preferences for contract Profile and cross sections sheets
Added Named Symbology - P_ALG_X DRAFTING NOTES
Drafting File added second station annotion for xsc 


