
8-17-2006 G. Sardinskas
Drainage cell levels in HW_plan.cel and HW_profile.cel were changed to wt. 4 from wt. 6.


9-19-2006 G.Sardinskas
All elements within the plan cells have been placed on: 
origins @ 0,0

9-21-2006 G.Sardinskas
New levels were created in the plan.cel file for scale bars 10 scale, 30 scale, 50 scale and 100 scale. All cells should have it's own level.
also new levels were created for HD-FEAT-RIVER, HD-FEAT-TIDAL, HD-SURF-CONC, HR-FEAT-BORING, HR-FEAT-EQUIV, HR-FEAT-HANDICAP, HR-FEAT-BOULDER

11-16-2006 E. Richard
ALL PUT ON CORRECT LEVEL
Bar Scale 20-1_pl
FLOW-RIVER_PL
FLOW-TIDAL_PL
BOULDER_PL
PATTERN_CONCRETE_PL
SYMBL-BORING_PL
SYMBL-EQUIV_PL
SYBL-HANDICAP_PL


11-17-2006 E. Richard
BAR SCALE 10-1_PL, (20-1) (30-1) (40-1) (50-1) (80-1) (100-1) (200-1) put on cooresponding level HB-CSHT-1inXXft.....

2-13-07 er
All text changed to Verdana

5-22-07 er
3 cable guiderail anchore Solid line changed form construction line to primary

09/24/09 er
Put text fields in ROW cell

