INI Revisions
XXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXX
May 3
created two separate v8 environments
2006 has leroy text
2007 has verdana + working text, new bdr size



Feb 7 2006
V3 
1.	Bin Report on Roadway Modeler turn off
2.	Bearings offset to bottom center 
3.	Feature for cut symb. Set for level HR_FEAT-cut
4.	BCLC feature line segments turned on in plan view
5.	Centerline feature line segments turn off in plan view
6.	Changed feature front of conc. Walk bench_rt to P_wlk, Sym P_buffer to breakline
7.	Updated tml
8.	Renamed INI to V4


Sept 25 2006
V4
1. Revised Options settings
	-Set A highway perference for UnitsTolerances Positional=1, Chord Height=1
		The default is set to .001 for chord ht as requested be surveys
	-Refesh command Settings on Preference Change ON
	-.12 decimal places set for N & E

2. Added symbology
	-P_ALG_H INTERSECTION COOR.
	-IND CON and INT CON
	-P_ALG H BEARING

3. Resised Horizantal Alignment Annotation
	-PI tangent turned off
	-Added NE PI coor to Curve data
	-PC STA. 10+00 changed to PC STA 10+00
	-Northing and Easting symbology set up.  Go to Geomentry>View Geometry>Station Base/clearance Annotation
	-Beaing set to standard

3. Revised all create cross section preferances
	-Station and elevation range off in create cross section and create profile
	-Cross section cell has a locked level so they can not be easily deleted
	-Create cross section features Include Features was turned ON
	-Window clearence forcross section, bottom changed to 15

4. Annotate profile revised
	-superelevation annotation was updated

5. Vertical annotation updated
	-Symbology is set for event Points

6. View surface updated
	-Added existing contour preference for veiwing contours

7. SURFACE > VEIW SURFACE 
	-Two point symbology annotation set

8. Existing Drainage Features
	-Added Profile symblogy and annotation for all existing drainage pipes and CBs
	-Added xsec symblogy and annotation for all existing drainage pipes, CB no option for project or ban with available in 8.5

9. Plan and Profile generator set up


Oct 02 2006
fwf and fxp v2
RevisionsOverhang chanded to exclude feature as dtm type.  


Nov 17 2006
ini V5
Separated CT Civil ini
Highways   CT_civil85_v5.ini - Set default perference for Units Tolerances Positional=1, Chord Height=1
		
surveys    SV_civil85_v5.ini - Set default perference for Units Tolerances Positional=1, Chord Height=.001


XXXXXXXXXXXXXXXXXXXXXXX MAY 3 XXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXXX


Jan 18, 2007
ini V6
Most fonts changed to Verdana, except existing features , Hor. and Vert. annotation
Highways   CT_civil85_v5.ini - Set default perference for Units Tolerances 
	Positional=.001, needed for annotating xsc
	Chord Height=1, needed for running modeler
Cleaned up preference manager


Jan 24 2007
Standard xsc preferance modified to accomodate the new bdr sheet along with rt & lt el and bottom symbology


Jan 28 2007
SV ini file updated with verdana design info chord ht set back to .001


April 2 2007
ini V7
Uppdated to CTDOT border Format 2007
	-created Plan Olnly 2007 and Profile Only 2007 for P&P Gen.
	-Changed new v to 7


April 30 2007
survey leroy to working, all leroy has be remove from INI


May 3
V7 changed all Verdana,1032 to verdana,229


May 15 2007
fwf and fxp v2
Jeff B - line style for edge of road


May 17 2007
fwf and fxp v3
John R all fonts to working

June 12 2007
fxp finished fonts to working


June 18 2007
John fixed fxp and fwf put V3 in 2006 and 2007
John fixed fxp and fwf in J envir
John fixed fxp and fwf in SE envir
Notes from John,
Feature level, weight, and color are in the FWF to bring in field data.
FXP controls how point info (num, code, elev, etc) is virtually displayed and also written to graphics.
However, the INI has final say for the notes using Named Symbology.
Placed features should take advantage of Named Symbology, but Surveys uses the bar menu to manually do everything, so that's why the ini was not apparent before.


Sept 21 2007
Version 8
S&S sym and features added for pipe, struc, area, ext.
Perimeter advance tab scale = 1 set for existing surface preference.

Nov 9 2007
Version 8a 
Saved xsc cell and 5 top margin to 2007 CTDOT Border Format 
Existing suface prefence set up for Contours


Jan 16 2008
civil Version 8b
Existing surface preference set to survey levels for Parimeter and Triangles
Default for Parimeter, Triangles, contour all set to sym o,o,o


Jan 22, 2008
Set existing surface per & Tria. by-levels for all attributes

Jan 25, 2008
civil Version 8c
Added Facility preferences for contract Profile and cross sections sheets
Added Named Symbology - P_ALG_X DRAFTING NOTES
Drafting File added second station annotion for xsc 
