**BED & SIDE RAIL SAFETY CHECKLIST**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Date:**      **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** **Name:**      **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** **Address:**      **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** | **Condition:****S – Satisfactory****U – Unsatisfactory, needs repair** | **Indicate action taken, if unsatisfactory**  |  | **Condition:****S – Satisfactory****U – Unsatisfactory, needs repair** | **Indicate action taken, if unsatisfactory** |
| **Bedframes and Rails** |  |  | **Mattress** |  |  |
| Clean | [ ]  **S**  [ ]  **U** |       | Fits properly | [ ]  **S**  [ ]  **U** |       |
| Rust free | [ ]  **S**  [ ]  **U** |       | Clean | [ ]  **S**  [ ]  **U** |       |
| No dents | [ ]  **S**  [ ]  **U** |       | No cracks/holes/rips | [ ]  **S**  [ ]  **U** |       |
| No sharp edges | [ ]  **S**  [ ]  **U** |       | No stains/odor | [ ]  **S**  [ ]  **U** |       |
| Mattress guard present | [ ]  **S**  [ ]  **U** |       | Gap between mattress and each side rail no more than 2 inches | [ ]  **S**  [ ]  **U** |       |
| Mattress guard in proper position | [ ]  **S**  [ ]  **U** |       |
| **Wooden Beds** |  |  | Headboard to mattress gap not more than 3 inches with bed flat | [ ]  **S**  [ ]  **U** |       |
| Finish Intact and Smooth  | [ ]  **S**  [ ]  **U** |       |
| **Semi-Electric and Fully Electric Beds** |  |  | Footboard to mattress no more than 3 inches | [ ]  **S**  [ ]  **U** |       |
| Cord/plug undamaged | [ ]  **S**  [ ]  **U** |       |
| Cord secured correctly | [ ]  **S**  [ ]  **U** |       | Gap between mattress and base of rails with HOB elevated 30 degrees no more than 3 inches | [ ]  **S**  [ ]  **U** |       |
| Controls work correctly | [ ]  **S**  [ ]  **U** |       |
| Grounded outlet used | [ ]  **S**  [ ]  **U** |       |
| **Bed Operations** |  |  | Distance between split in split rail configurations not more than 12.5 inches | [ ]  **S**  [ ]  **U** |       |
| Cranks smoothly | [ ]  **S**  [ ]  **U** |       | **Egg crate foam/****Air Mattress** |  |  |
| Wheels operate smoothly | [ ]  **S**  [ ]  **U** |       | Clean | [ ]  **S**  [ ]  **U** |       |
| Wheel lock works | [ ]  **S**  [ ]  **U** |       | No cracks/holes/rips | [ ]  **S**  [ ]  **U** |       |
| Headboard secured | [ ]  **S**  [ ]  **U** |       | No stains/odors | [ ]  **S**  [ ]  **U** |       |
| Footboard secured | [ ]  **S**  [ ]  **U** |       |  |  |  |
|  |  |  |  |  |  |

**BED & SIDE RAIL SAFETY CHECKLIST**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Date:**      **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** **Name:**      **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** **Address:**      **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** | **Condition:****S – Satisfactory****U – Unsatisfactory, needs repair** | **Indicate action taken, if unsatisfactory**  |  | **Condition:****S – Satisfactory****U – Unsatisfactory, needs repair** | **Indicate action taken, if unsatisfactory** |
| **Side Rails** |  |       | **Side Rail Pads** |  |  |
| No play detected | [ ]  **S**  [ ]  **U** |       | Clean | [ ]  **S**  [ ]  **U** |       |
| Operate correctly | [ ]  **S**  [ ]  **U** |       | No cracks/holes/rips | [ ]  **S**  [ ]  **U** |       |
| Not bowed or warped | [ ]  **S**  [ ]  **U** |       | No stains/odor | [ ]  **S**  [ ]  **U** |       |
| Distance b/w mattress & headboard same as distance b/w mattress & footboard? | [ ]  **S**  [ ]  **U** |       |  |  |  |
| Distance b/w mattress & side rail on Right side same as distance b/w mattress & side rail on Left side? | [ ]  **S**  [ ]  **U** |       |  |  |  |
|  |
| **Name and Signature of Person Completing Checklist:**      **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** |